(module ITDB02-3.2WD (layer F.Cu) (tedit 56C57F94)
  (fp_text reference REF** (at -0.8 -3.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ITDB02-3.2WD (at 9.2 -3.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 240px (at 77 26) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 400px (at 43.3 5.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 3.2" (at 43.9 25.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9 49.9) (end 80 4) (layer F.SilkS) (width 0.15))
  (fp_line (start 9 49.9) (end 9 4) (layer F.SilkS) (width 0.15))
  (fp_line (start 80 50) (end 9 49.9) (layer F.SilkS) (width 0.15))
  (fp_line (start 80 4) (end 80 50) (layer F.SilkS) (width 0.15))
  (fp_line (start 9 4) (end 80 4) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 56.8) (end -3 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 92 56.8) (end -3 56.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 92 -3) (end 92 56.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -3) (end 92 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.85 1.0246) (end -1.85 52.8246) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.2 1.0246) (end 4.2 52.8246) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.85 1.0246) (end 4.2 1.0246) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.85 52.8246) (end 4.2 52.8246) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.71 52.3046) (end 3.71 1.5046) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.37 4.0446) (end -1.37 52.3046) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.71 52.3046) (end -1.37 52.3046) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.71 1.5046) (end 1.17 1.5046) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.1 1.2246) (end -1.65 1.2246) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.17 1.5046) (end 1.17 4.0446) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.17 4.0446) (end -1.37 4.0446) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.65 1.2246) (end -1.65 2.7746) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at -0.1 2.7746) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole oval (at 2.44 2.7746) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole oval (at -0.1 5.3146) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole oval (at 2.44 5.3146) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole oval (at -0.1 7.8546) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole oval (at 2.44 7.8546) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole oval (at -0.1 10.3946) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole oval (at 2.44 10.3946) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 9 thru_hole oval (at -0.1 12.9346) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole oval (at 2.44 12.9346) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 11 thru_hole oval (at -0.1 15.4746) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 12 thru_hole oval (at 2.44 15.4746) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 13 thru_hole oval (at -0.1 18.0146) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 14 thru_hole oval (at 2.44 18.0146) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 15 thru_hole oval (at -0.1 20.5546) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 16 thru_hole oval (at 2.44 20.5546) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 17 thru_hole oval (at -0.1 23.0946) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 18 thru_hole oval (at 2.44 23.0946) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 19 thru_hole oval (at -0.1 25.6346) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 20 thru_hole oval (at 2.44 25.6346) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 21 thru_hole oval (at -0.1 28.1746) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 22 thru_hole oval (at 2.44 28.1746) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 23 thru_hole oval (at -0.1 30.7146) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 24 thru_hole oval (at 2.44 30.7146) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 25 thru_hole oval (at -0.1 33.2546) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 26 thru_hole oval (at 2.44 33.2546) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 27 thru_hole oval (at -0.1 35.7946) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 28 thru_hole oval (at 2.44 35.7946) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 29 thru_hole oval (at -0.1 38.3346) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 30 thru_hole oval (at 2.44 38.3346) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 31 thru_hole oval (at -0.1 40.8746) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 32 thru_hole oval (at 2.44 40.8746) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 33 thru_hole oval (at -0.1 43.4146) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 34 thru_hole oval (at 2.44 43.4146) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 35 thru_hole oval (at -0.1 45.9546) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 36 thru_hole oval (at 2.44 45.9546) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 37 thru_hole oval (at -0.1 48.4946) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 38 thru_hole oval (at 2.44 48.4946) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 39 thru_hole oval (at -0.1 51.0346) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 40 thru_hole oval (at 2.44 51.0346) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 9 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 9 53.8) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 80 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at 80 53.8) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
    (at (xyz 0.05 -0.95 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
